|  |  |
| --- | --- |
| Author Name: Kevin Arne Title: Prototyping Labs Supervisor  Date: 4/13/2022 | |
| #1 Process  (if applicable) |  |
| #2 Equipment | ProtoLaser U4 |
| #3 Personal Protective Equipment (PPE) | * Eye protection |
| #4 Environmental /  Ventilation controls. |  |
| #5 Required training or approval | * Review and observe general safety practices outlined in the Shop Equipment Safety Guidelines. * Refer to the manufacturer’s operating manual for all operating procedures. |
| #6 Inspection requirements before use | * Visually inspect the tool for damage. |
| #7 Safe operating procedures or precautions | * Make sure that dust extraction is activated during machining of the work piece. Use fine particle filters exclusively. |
| #8 Chemicals/ spill procedures/waste disposal |  |
| Author Signature: Date: | |